|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| KNCSHY74CCK617298 | 봉고 III 1TON,1.4TON,4W(BONGO III):NOV.2006- | KOREA,SOUTH | 2011/09/20 | 4 |  | HDH98A856 | SA20 | 01 |

 |  | [SEARCH](http://wpc.mobis.co.kr/ModelSearch?cmd=search&mode=first&Json=N) |   |

|  |
| --- |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|   |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Model No | HDH98A856 | Engine No | J3 B 138343 | T/M No |  | P/Catalog Name |
| Exterior Color1 |   MA    | Engine MIP | K95V | T/M MIP | EH | KDOMPPU04 | 봉고 III 1TON,1.4TON,4W(BONGO III):NOV.2006- |
| Exterior Color2 |   MA    | Body | 1T H/LONG DBL | Engine Capacity | 2.9L-J3 | Engine | SOHC-TCI | Special Car |  |
| Interior Color |   GW                     | Fuel | DIESEL | T/M | 5MT4WD | Drive Type | LHD | ADDON |  |

 |

|  |  |
| --- | --- |
| 2811A1 | INTAKE TYPE - SNORKEL TYPE |
| 2821A1 | T/C CAUTION LABEL - KOREAN |
| 2842A1 | EMISSION CONTROL SYSTEM - E.G.R. |
| 3111C1 | FUEL TANK-CAPACITY - 60 LITER |
| 3241A2 | FUEL ECONOMY LABEL - KOREA LANGUAGE |
| 3311A2 | PUMP CONTROL - ELECTRONIC TYPE |
| 3711B8 | BATTERY CAPACITY - 80AH (5HR) |
| 371CA1 | BATTERY SAVER |
| 3914A1 | F.F.H.S(FUEL FILTER HEAT`G) |
| 4371A1 | MT KNOB - SOFT PVC |
| 4501A1 | CLUTCH LOCK |
| 5171A2 | INDEPENDENT - 6 SIZE |
| 5291G3 | STEEL WHEEL - 5.5J \* 15 5.5J \* 15 |
| 5293E9 | 195 TIRE - 195/R15 8PR 195 R15-8PR |
| 5297A1 | FULL SIZE 1EA - STEEL WHEEL & TIRE |
| 5299A1 | SPARE TIRE LOCK`G SYSTEM |
| 529TA1 | TOOL SET & JACK LABEL - KOREA |
| 5415A1 | TORSION BAR SPRING |
| 5511A7 | RR SUSP TYPE - LEAF SPRING-GENERAL TYPE |
| 5531A2 | TUN`G MODE - HARD SUSPENSION |
| 5611B2 | 3-SPOKE - POLY URETHANE |
| 5631A1 | STEER`G COLUMN-NON-TILT |
| 5711A2 | HPS(HYDRAULIC POWER STRG) |
| 5811A3 | FR BRAKE - DISC-14 INCH |
| 5812A2 | RR BRAKE - DRUM-8 INCH |
| 5911B1 | TANDEM BOOSTER - 8+9 INCH |
| 6311A1 | CAB MTG TYPE - NON-TILTING |
| 6501A2 | LOW GRADE |
| 8152A2 | FUEL FILLER DR REL TYPE - KEY |
| 8232A1 | UPR TRIM FINISH`G - PLASTIC(NO COVER`G) |
| 8235A1 | MAP POCKET FINISH`G - W/O T/C PILE |
| 8236A1 | ARM REST COVER`G - PVC |
| 8241A1 | FR DR GLASS - CLEAR |
| 8245A1 | RR DR GLASS - CLEAR |
| 8261A1 | FINISH`G - BLACK COLOR |
| 8421B1 | LINOLEUM |
| 842BA1 | FOOT REST - METAL |
| 8431C2 | CAR MAT - PVC |
| 8441A3 | FR - ASH TRAY W/ ILLUM |
| 8445A1 | CIGAR LIGHTER - W/O ILLUM. |
| 8451A1 | W/O LOCK |
| 8475A1 | CUP HOLDER - SEPARATE |
| 8491A1 | CTR FACIA PNL |
| 84B5A1 | SMALL TRAY |
| 84K4A1 | MULTI MINI POCKET |
| 8511A1 | STD TYPE |
| 8521A1 | MATERIAL - VINYL |
| 8523A1 | MATERIAL - VINYL |
| 8531A2 | ROOF TRIM MATERIAL - FABRIC |
| 8532A1 | FR - 1 EA |
| 8534A2 | FR - 2 EA |
| 853AA2 | RR - 2 EA |
| 8581B2 | FORMED TYPE - PLASTIC |
| 8611A1 | W/S GLASS TYPE-CLEAR (W/O S/BAND) |
| 8621A1 | BODY SIDE |
| 863CA0 | GRADE - L |
| 8641A1 | TOWING HOOK |
| 8649A8 | ID PLATE - KOREAN TYPE |
| 8651A1 | TYPE - GENERAL |
| 865CA1 | RR GUARD & PROTECTOR - RR GUARD |
| 8681A1 | MUD GUARD-FR |
| 8712A1 | BACK LITE GLASS TYPE -CLEAR(W/O HEATED) |
| 8761B1 | QUADRANT - BALL TYPE |
| 8765A1 | COLOR - BLACK |
| 8811F3 | ARTIFICIAL LEATHER - TWO TONE |
| 8821A1 | HEAD REST - UP/DOWN |
| 8823A1 | SLIDING |
| 8824A2 | DOUBLE RECLIN`G |
| 8852A2 | FOR 2 PEOPLE - BENCH-FOLD`G |
| 8854A1 | HEAD REST - UP/DOWN |
| 885EA2 | DOUBLE RECLIN`G |
| 8872A1 | SEAT BACK CONSOLE - SEAT BACK CONSOLE |
| 8881B1 | DRIVER`S SIDE - ELR |
| 8883A1 | CTR-STATIC |
| 8884D1 | PASSENGER`S SIDE - ELR |
| 8981A1 | SIDE - STATIC |
| 8982A1 | CTR - STATIC |
| 9211E3 | MFR - CLEAR |
| 9232A1 | CONVENTIONAL - CLEAR LENS |
| 9241A2 | NON LED TYPE |
| 9281A1 | ROOM LAMP-FR(GLOW LAMP) |
| 928FA1 | CTR - GLOW LAMP |
| 928WA2 | BULB TYPE - 2 BULB |
| 92HCA1 | DELAY LAMP |
| 9402A1 | SPEEDOMETER |
| 940BA1 | TACHOMETER |
| 940CA1 | FUEL |
| 940DA1 | WATER TEMP. |
| 9451A1 | TYPE - DIGITAL |
| 94C6A1 | DIRECTION INDICATOR |
| 94C7A1 | OIL PRESSURE |
| 94C9A1 | PARK`G BRAKE |
| 94D0A1 | DR AJAR - DR AJAR |
| 94D1A1 | BATTERY CHARGE |
| 94D4A1 | LOW FUEL |
| 94D9A1 | CHECK ENGINE |
| 94E3A1 | SEAT BELT |
| 94G5A1 | GLOW INDICATOR |
| 94M0A1 | SPEEDOMETER TYPE - KMPH |
| 94N0A1 | TEMPERATURE UNIT - C |
| 9541A2 | BODY CONTROL MODULE - T.A.C.U |
| 9545A1 | FREQUENCY-SMART KEY - DOMESTIC |
| 9615A1 | FREQUENCY VIBRATION - AM9K/FM100K |
| 9621A1 | ANTENNA TELESCOPIC - MANUAL |
| 9631A1 | SPEAKER CAPACITY - 2 EA |
| 9661A1 | HORN - SINGLE |
| 9713A2 | PTC HEATER\_INT TYPE |
| 9714B1 | FUNCTION - DUST FILTER |
| 9721A2 | CABLE TYPE - ROTARY TYPE |
| 9811A2 | FR WIPER - INTERMITTENT(VARIABLE) |
| 981AA1 | FR WIPER-2 SPEED |
| WT 3 |   |

|  |  |
| --- | --- |
| 2841M5 | EMISSION REGULATION - DOM EURO 4 |
| 2891C1 | CATALYTIC CONVERTER - W.C.C+U.C.C TYPE |
| 5272A3 | RR AXLE FUNCTION -L.D LOCKG DEFERENTIAL |
| 5296C1 | FULL SIZE WHL COVER - A TYPE |
| 6111A1 | RR DECK MATERIAL - STEEL |
| 6112A1 | BRIM COVER |
| 8131A2 | CENTRAL DR LOCK/UNLOCK-DR`S & PA`S CTRL |
| 8194B3 | TYPE - FOLDING |
| 819FA1 | KEYLESS ENTRY-CENTRAL LOCK |
| 8233A1 | CENTER TRIM - PLASTIC(NO COVER`G) |
| 8341A1 | POWER WINDOW(FR) |
| 834AA1 | AUTO DOWN |
| 8494A1 | P/WINDOW SW PNL |
| 8652B1 | COLOR - BODY COLOR |
| 8682A1 | MUD GUARD-RR |
| 8762C4 | PASS`S SIDE - ELECTRIC HTD-CONV |
| 8763C4 | DRIVER`S SIDE - ELECTRIC HTD-CONV |
| 8768A1 | FR UNDER VIEW MIRROR |
| 8838A1 | SEAT WARMER(HEATER) |
| 9221D1 | CONVENTIONAL - CLEAR |
| 928HA2 | FR - REFLECTOR |
| 9611H5 | RADIO+CD - K 260 |
| 9761A1 | FR COOLER - MANUAL A/CON |
| A99 | KOREA,SOUTH |